**Pop-Up Float Burn Wire Release Specifications Sheet**

* Programmable timed burn wire release
* Salt water submersible up to minimum 300m depth
* Minimum 300lb working load with a 600lb max breaking strength
* Capable to program burn time up to 24 months from program date
* Burn wire activated by 18V battery pack (two 9V batteries in series, not required to be provided by vendor- only the voltage specification applies here)
* Burn time averages between 8 to 16 minutes
* Circuit board switch connected to burn wire release via 7/16” 20 TPI bulkhead connector/penetrator
* Cables to connect burn wire release to bulkhead connector/penetrator must be 17”
* Functional in temperatures at least between -5 °C and 15°C